# Errata: Coherent Components

## SYSCOREQ handshaking for ACE master

If using a Netspeed provided voltage-domain crossing with an ACE master, and using a Qchannel to control power-management, then SYSCOREQ shall not be asserted until the Qchannel handshake has reached the Q\_RUN state.