# Changes to Commands and Properties

## Command Changes

|  |  |
| --- | --- |
| **Command Name** | **Comment** |
| add\_output\_reg\_across\_rtl\_group | Name change. Previous name was add\_output\_reg\_across\_rtlgroup |
| show\_project | New command to print the project name |
| map | This command has been deprecated |
| tune\_route | This command has been deprecated |
| tune\_links | This command has been deprecated |

## Default Property Changes

|  |  |  |
| --- | --- | --- |
| **Property Name** | **Default Value** | **Comment** |
| msg\_peak\_bw | 6.4 | This property has been deprecated |
| msg\_peak\_rate | 0.1 | This property has been deprecated |
| peak\_multiplier | 1 | New property to specify the default multiplier to calculate peak rate/bw from average rate/bw when the peak rate/bw is not specified |
| read\_burstiness | 1 | The default value for this property has been changed from 3 to 1 |

## Mesh Property Changes

|  |  |  |
| --- | --- | --- |
| **Property Name** | **Default Value** | **Comment** |
| compact\_regbus\_address\_space | Yes | Default value of this property has changed from No to Yes |
| extra\_bandwidth\_provisioning | 0 | Default value of this property has changed from 25 to 0 |
| stats\_level | High | New property to specify the default level of statistics collection in NocStudio performance simulator |

## Bridge Property Changes

None

## Host Property Changes

None

## Interface Property Changes

|  |  |
| --- | --- |
| **Property Name** | **Comment** |
| initial\_credits | This property has been deprecated. |

## Link Property Changes

None

## Router Property Changes

None

## VC Property Changes

None