# Errata

## Synthesis results with Multi Cell Size NoCs

It has been observed that the synthesis tools do not propagate constants defined in the RTL code properly for some configuration with multi cell\_size option. This results in dividers being instantiated in the netlist and reducing the achievable frequency. Please contact NetSpeed Support team if your design intends to implement multi cell size NoC.