# Changes to Commands and Properties

## Command Changes

|  |  |
| --- | --- |
| **Property Name** | **Comment** |
| add\_regbus\_controller | This command adds a Regbus Controller (RBC) with its RBM and optional Axi4s bridge to tunnel requests from masters in the NoC, or APBM| AXI4LM| IOSFSB| IOSFSB2APB interfaces to drive external requests into the RBC. |
| vifce\_prop | This command is used to set or view a named property of a particular Interface's virtual interface and an optional direction in/out, w.r.t the host. |
| reset\_mesh | This command resets the previously created mesh. |

## Default Property Changes

None

## Mesh Property Changes

None

## Bridge Property Changes

None

## Host Property Changes

None

## Interface Property Changes

None

## Link Property Changes

None

## Router Property Changes

None

## VC Property Changes

None

## CSB Storage Property Changes

None